

PLX9080
PLX9054

SEEPROM Offset
Description
SEEPROM Value

[HiB][LoB]
SEEPROM Value [HiB][LoB]

0h
Device ID   [PCIIDR(31-16)]
9080
9054

2h
Vendor ID   [PCIIDR(15-0)]
10B5
10B5

4h
Class Code  [PCICCR(23-9)]
0680
0680

6h
Class Code Revision  [PCICCR(7-0) / PCIREV(7-0)]
0002
000C

8h
Maximum Latency, Minimum Grant [PCIMLR(70)/PCIMGR(7-0)]
0000
0000

Ah
Interrupt Pin, Interrupt Line Routing [PCIIPR(7-0)/PCIILR(7-0)]
0100
0100

Ch
MSW of Mailbox 0 (User Defined) [MBOX0(31-16)]
0000
0000

Eh
LSW of Mailbox 0 (User Defined) [MBOX0(15-0)]
0000 
0000

10h
MSW of Mailbox 1 (User Defined) [MBOX1(31-16)]
0000
0000

12h
LSW of Mailbox 1 (User Defined) [MBOX1(15-0)]
0000
0000

14h
MSW of Range for PCI-to-Local Address Space 0 [LASORR(31-16)]
FFF0
FFE0

16h
LSW of Range for PCI-to-Local Address Space 0 [LASORR(15-0)]
0000
0000

18h
MSW of Local Base Address (Remap) for PCI-to-Local Address Space 0 [LASOBA(31-16)]
0000
0000

1Ah
LSW of Local Base Address (Remap) for PCI-to-Local Address Space 0 [LASOBA(15-0)]
0001
0001

1Ch
MSW of Local Arbitration Register [MARBR(31-16)]
0000
0000

1Eh
LSW of Local Arbitration Register [MARBR(15-0)]
0000
0000        

20h
MSW of Serial EEPROM Write-Protected Address 

[PROT_AREA(15-0)]
0000
0030                       

22h
LSW of Local Miscellaneous Control Register/ LSW of Local Bus Big/Little

 Endian Descriptor Reg  [LMISC(7-0)/BIGEND(7-0)]
0000
0500

24h
MSW of Range for PCI-to-Local Expansion ROM [EROMRR(31-16)]
0000
0000

26h
LSW of Range for PCI-to-Local Expansion ROM  [EROMRR(15-0)]
0000
0000

28h
MSW of Local Base Address (Remap) for PCI-to-Local Expansion ROM

 [EROMBA(31-16)]
0000
0000

2Ah
LSW of Local Base Address (Remap) for PCI-to-Local Expansion ROM

[EROMBA(15-0)]
0000
0000

2Ch
MSW of Bus Region Descriptors for PCI-to-Local Accesses

 [LBRDO(31-16)]
0000
0000 

2Eh
LSW of Bus Region Descriptors for PCI-to-Local Accesses

 [LBRDO(15-0)]
0000
0043

...
.................
0000
0000

...
.................
0000
0000

42h
LSW of PCI Configuration Address Register for PCI Initiator-to-PCI I/O Configuration [DMCFGA(15-0)]
0000
0000

SERIAL EEPROM  NM93CS46/56/66L








